**HD800 Specification**

|  |  |
| --- | --- |
| Images Sensors: | OV2710 CCD |
| Video resolution | 1080P |
| CCD Video resolution | Telephoto small distortion lens |
| Digital Program | V3S |
| Video Compressing Format | H.264 |
| Video File Format | MOV |
| Photo Format | JEP |
| Photo Size | 4000\*3000 |
| [Microphone](file:///C:\Users\Administrator\AppData\Local\youdao\dict\Application\7.0.1.0214\resultui\dict\result.html?keyword=microphone) | Built-in microphone |
| USB Interface | USB 2.0 |
| LCD screen | 1.5 inch, resolution: 320\*240 |
| Storage | Micro SD card 16GB |
| Battery Specification | 3.7V Rechargeable lithium batteries, 10000mAH |
| dB | >48dB |
| [Relative](file:///C:\Users\Administrator\AppData\Local\youdao\dict\Application\7.0.1.0214\resultui\dict\result.html?keyword=relative) [Humidity](file:///C:\Users\Administrator\AppData\Local\youdao\dict\Application\7.0.1.0214\resultui\dict\result.html?keyword=humidity) | 5%~95%RH |
| Storage temperature | -20~70℃ |
| Working Temperature | -10~ 50 ℃ |
| Power | 5W |
|  |  |
| Net Weight | 555g |
|  |  |
| Gross Weight | 1416g |
|  |  |